Skip to content

# Modules Options

> This section describes modules options of ejabberd 24.07. If you are using an old ejabberd release, please refer to the corresponding archived version of this page in the Archive. The modules that changed in this version are marked with 🟤.

## mod_adhoc

This module implements XEP-0050: Ad-Hoc Commands. It’s an auxiliary module and is only needed by some of the other modules.

Available options:

- report_commands_node: true | false
  Provide the Commands item in the Service Discovery. Default value: false.

## mod_admin_extra

This module provides additional administrative commands.

Details for some commands:

- ban_account: This command kicks all the connected sessions of the account from the server. It also changes their password to a randomly generated one, so they can’t login anymore unless a server administrator changes their password again. It is possible to define the reason of the ban. The new password also includes the reason and the date and time of the ban. See an example below.

- pushroster: (and pushroster-all) The roster file must be placed, if using Windows, on the directory where you installed ejabberd: `C:/Program Files/ejabberd` or similar. If you use other Operating System, place the file on the same directory where the .beam files are installed. See below an example roster file.

- srg_create: If you want to put a group Name with blank spaces, use the characters "' and '" to define when the Name starts and ends. See an example below.

The module has no options.

Examples:

With this configuration, vCards can only be modified with mod_admin_extra commands:

    acl:
      adminextraresource:
        - resource: "modadminextraf8x,31ad"
    access_rules:
      vcard_set:
        - allow: adminextraresource
    modules:
      mod_admin_extra: {}
      mod_vcard:
        access_set: vcard_set

Content of roster file for pushroster command:

    [{<<"bob">>, <<"example.org">>, <<"workers">>, <<"Bob">>},
    {<<"mart">>, <<"example.org">>, <<"workers">>, <<"Mart">>},
    {<<"Rich">>, <<"example.org">>, <<"bosses">>, <<"Rich">>}].

With this call, the sessions of the local account which JID is boby@example.org will be kicked, and its password will be set to something like BANNED_ACCOUNT—20080425T21:45:07—2176635—Spammed_rooms

    ejabberdctl vhost example.org ban_account boby "Spammed rooms"

Call to srg_create using double-quotes and single-quotes:

    ejabberdctl srg_create g1 example.org "'Group number 1'" this_is_g1 g1

## mod_admin_update_sql

This module can be used to update existing SQL database from the default to the new schema. Check the section Singlehost or Multihost for details. Please note that only MS SQL, MySQL, and PostgreSQL are supported. When the module is loaded use update_sql API.

The module has no options.

## mod_announce

This module enables configured users to broadcast announcements and to set the message of the day (MOTD). Configured users can perform these actions with an XMPP client either using Ad-hoc Commands or sending messages to specific JIDs.

Note that this module can be resource intensive on large deployments as it may broadcast a lot of messages. This module should be disabled for instances of ejabberd with hundreds of thousands users.

The Ad-hoc Commands are listed in the Server Discovery. For this feature to work, mod_adhoc must be enabled.

The specific JIDs where messages can be sent are listed below. The first JID in each entry will apply only to the specified virtual host example.org, while the JID between brackets will apply to all virtual hosts in ejabberd:

- example.org/announce/all (example.org/announce/all-hosts/all):: The message is sent to all registered users. If the user is online and connected to several resources, only the resource with the highest priority will receive the message. If the registered user is not connected, the message will be stored offline in assumption that offline storage (see mod_offline) is enabled.

- example.org/announce/online (example.org/announce/all-hosts/online):: The message is sent to all connected users. If the user is online and connected to several resources, all resources will receive the message.

- example.org/announce/motd (example.org/announce/all-hosts/motd):: The message is set as the message of the day (MOTD) and is sent to users when they login. In addition the message is sent to all connected users (similar to announce/online).

- example.org/announce/motd/update (example.org/announce/all-hosts/motd/update):: The message is set as message of the day (MOTD) and is sent to users when they login. The message is not sent to any currently connected user.

- example.org/announce/motd/delete (example.org/announce/all-hosts/motd/delete):: Any message sent to this JID removes the existing message of the day (MOTD).

Available options:

- access: AccessName
  This option specifies who is allowed to send announcements and to set the message of the day. The default value is none (i.e. nobody is able to send such messages).

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

## mod_avatar

The purpose of the module is to cope with legacy and modern XMPP clients posting avatars. The process is described in XEP-0398: User Avatar to vCard-Based Avatars Conversion.

Also, the module supports conversion between avatar image formats on the fly.

The module depends on mod_vcard, mod_vcard_xupdate and mod_pubsub.

Available options:

- convert: {From: To}
  Defines image conversion rules: the format in From will be converted to format in To. The value of From can also be default, which is match-all rule. NOTE: the list of supported formats is detected at compile time depending on the image libraries installed in the system.

  Example:

      convert:
        webp: jpg
        default: png

- rate_limit: Number
  Limit any given JID by the number of avatars it is able to convert per minute. This is to protect the server from image conversion DoS. The default value is 10.

## mod_block_strangers

This module blocks and logs any messages coming from an unknown entity. If a writing entity is not in your roster, you can let this module drop and/or log the message. By default you’ll just not receive message from that entity. Enable this module if you want to drop SPAM messages.

Available options:

- access: AccessName
  The option is supposed to be used when allow_local_users and allow_transports are not enough. It’s an ACL where deny means the message will be rejected (or a CAPTCHA would be generated for a presence, if configured), and allow means the sender is whitelisted and the stanza will pass through. The default value is none, which means nothing is whitelisted.

- allow_local_users: true | false
  This option specifies if strangers from the same local host should be accepted or not. The default value is true.

- allow_transports: true | false
  If set to true and some server’s JID is in user’s roster, then messages from any user of this server are accepted even if no subscription present. The default value is true.

- captcha: true | false
  Whether to generate CAPTCHA or not in response to messages from strangers. See also section CAPTCHA of the Configuration Guide. The default value is false.

- drop: true | false
  This option specifies if strangers messages should be dropped or not. The default value is true.

- log: true | false
  This option specifies if strangers' messages should be logged (as info message) in ejabberd.log. The default value is false.

## mod_blocking

The module implements XEP-0191: Blocking Command.

This module depends on mod_privacy where all the configuration is performed.

The module has no options.

## mod_bosh

This module implements XMPP over BOSH as defined in XEP-0124 and XEP-0206. BOSH stands for Bidirectional-streams Over Synchronous HTTP. It makes it possible to simulate long lived connections required by XMPP over the HTTP protocol. In practice, this module makes it possible to use XMPP in a browser without WebSocket support and more generally to have a way to use XMPP while having to get through an HTTP proxy.

Available options:

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- json: true | false
  This option has no effect.

- max_concat: pos_integer() | infinity
  This option limits the number of stanzas that the server will send in a single bosh request. The default value is unlimited.

- max_inactivity: timeout()
  The option defines the maximum inactivity period. The default value is 30 seconds.

- max_pause: pos_integer()
  Indicate the maximum length of a temporary session pause (in seconds) that a client can request. The default value is 120.

- prebind: true | false
  If enabled, the client can create the session without going through authentication. Basically, it creates a new session with anonymous authentication. The default value is false.

- queue_type: ram | file
  Same as top-level queue_type option, but applied to this module only.

- ram_db_type: mnesia | sql | redis
  Same as top-level default_ram_db option, but applied to this module only.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

Example:

    listen:
      -
        port: 5222
        module: ejabberd_c2s
      -
        port: 5443
        module: ejabberd_http
        request_handlers:
          /bosh: mod_bosh

    modules:
      mod_bosh: {}

## mod_caps

This module implements XEP-0115: Entity Capabilities. The main purpose of the module is to provide PEP functionality (see mod_pubsub).

Available options:

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

## mod_carboncopy

The module implements XEP-0280: Message Carbons. The module broadcasts messages on all connected user resources (devices).

The module has no options.

## mod_client_state

This module allows for queueing certain types of stanzas when a client indicates that the user is not actively using the client right now (see XEP-0352: Client State Indication). This can save bandwidth and resources.

A stanza is dropped from the queue if it’s effectively obsoleted by a new one (e.g., a new presence stanza would replace an old one from the same client). The queue is flushed if a stanza arrives that won’t be queued, or if the queue size reaches a certain limit (currently 100 stanzas), or if the client becomes active again.

Available options:

- queue_chat_states: true | false
  Queue "standalone" chat state notifications (as defined in XEP-0085: Chat State Notifications) while a client indicates inactivity. The default value is true.

- queue_pep: true | false
  Queue PEP notifications while a client is inactive. When the queue is flushed, only the most recent notification of a given PEP node is delivered. The default value is true.

- queue_presence: true | false
  While a client is inactive, queue presence stanzas that indicate (un)availability. The default value is true.

## mod_configure

The module provides server configuration functionality via XEP-0050: Ad-Hoc Commands. Implements many commands as defined in XEP-0133: Service Administration. This module requires mod_adhoc to be loaded.

The module has no options.

## mod_conversejs

added in 21.12 and improved in 22.05

This module serves a simple page for the Converse XMPP web browser client.

To use this module, in addition to adding it to the modules section, you must also enable it in listen → ejabberd_http → request_handlers.

Make sure either mod_bosh or ejabberd_http_ws request_handlers are enabled.

When conversejs_css and conversejs_script are auto, by default they point to the public Converse client.

Available options:

- bosh_service_url: auto | BoshURL
  BOSH service URL to which Converse can connect to. The keyword @HOST@ is replaced with the real virtual host name. If set to auto, it will build the URL of the first configured BOSH request handler. The default value is auto.

- conversejs_css: auto | URL
  Converse CSS URL. The keyword @HOST@ is replaced with the hostname. The default value is auto.

- conversejs_options: {Name: Value}
  added in 22.05 Specify additional options to be passed to Converse. See Converse configuration. Only boolean, integer and string values are supported; lists are not supported.

- conversejs_resources: Path
  added in 22.05 Local path to the Converse files. If not set, the public Converse client will be used instead.

- conversejs_script: auto | URL
  Converse main script URL. The keyword @HOST@ is replaced with the hostname. The default value is auto.

- default_domain: Domain
  Specify a domain to act as the default for user JIDs. The keyword @HOST@ is replaced with the hostname. The default value is @HOST@.

- websocket_url: auto | WebSocketURL
  A WebSocket URL to which Converse can connect to. The keyword @HOST@ is replaced with the real virtual host name. If set to auto, it will build the URL of the first configured WebSocket request handler. The default value is auto.

Examples:

Manually setup WebSocket url, and use the public Converse client:

    listen:
      -
        port: 5280
        module: ejabberd_http
        request_handlers:
          /bosh: mod_bosh
          /websocket: ejabberd_http_ws
          /conversejs: mod_conversejs

    modules:
      mod_bosh: {}
      mod_conversejs:
        websocket_url: "ws://@HOST@:5280/websocket"

Host Converse locally and let auto detection of WebSocket and Converse URLs:

    listen:
      -
        port: 443
        module: ejabberd_http
        tls: true
        request_handlers:
          /websocket: ejabberd_http_ws
          /conversejs: mod_conversejs

    modules:
      mod_conversejs:
        conversejs_resources: "/home/ejabberd/conversejs-9.0.0/package/dist"

Configure some additional options for Converse

    modules:
      mod_conversejs:
        websocket_url: auto
        conversejs_options:
          auto_away: 30
          clear_cache_on_logout: true
          i18n: "pt"
          locked_domain: "@HOST@"
          message_archiving: always
          theme: dracula

## mod_delegation

This module is an implementation of XEP-0355: Namespace Delegation. Only admin mode has been implemented by now. Namespace delegation allows external services to handle IQ using specific namespace. This may be applied for external PEP service.

> Warning

> Security issue: Namespace delegation gives components access to sensitive data, so permission should be granted carefully, only if you trust the component.

> Note

> This module is complementary to mod_privilege but can also be used separately.

Available options:

- namespaces: {Namespace: Options}
  If you want to delegate namespaces to a component, specify them in this option, and associate them to an access rule. The Options are:

  - access: AccessName
    The option defines which components are allowed for namespace delegation. The default value is none.

  - filtering: Attributes
    The list of attributes. Currently not used.

Examples:

Make sure you do not delegate the same namespace to several services at the same time. As in the example provided later, to have the sat-pubsub.example.org component perform correctly disable the mod_pubsub module.

    access_rules:
      external_pubsub:
        allow: external_component
      external_mam:
        allow: external_component

    acl:
      external_component:
        server: sat-pubsub.example.org

    modules:
      mod_delegation:
        namespaces:
          urn:xmpp:mam:1:
            access: external_mam
          http://jabber.org/protocol/pubsub:
            access: external_pubsub

## mod_disco

This module adds support for XEP-0030: Service Discovery. With this module enabled, services on your server can be discovered by XMPP clients.

Available options:

- extra_domains: [Domain, ...]
  With this option, you can specify a list of extra domains that are added to the Service Discovery item list. The default value is an empty list.

- name: Name
  A name of the server in the Service Discovery. This will only be displayed by special XMPP clients. The default value is ejabberd.

- server_info: [Info, ...]
  Specify additional information about the server, as described in XEP-0157: Contact Addresses for XMPP Services. Every Info element in the list is constructed from the following options:

  - modules: all | [Module, ...]
    The value can be the keyword all, in which case the information is reported in all the services, or a list of ejabberd modules, in which case the information is only specified for the services provided by those modules.

  - name: Name
    The field var name that will be defined. See XEP-0157 for some standardized names.

  - urls: [URI, ...]
    A list of contact URIs, such as HTTP URLs, XMPP URIs and so on.

  Example:

      server_info:
        -
          modules: all
          name: abuse-addresses
          urls: ["mailto:abuse@shakespeare.lit"]
        -
          modules: [mod_muc]
          name: "Web chatroom logs"
          urls: ["http://www.example.org/muc-logs"]
        -
          modules: [mod_disco]
          name: feedback-addresses
          urls:
            - http://shakespeare.lit/feedback.php
            - mailto:feedback@shakespeare.lit
            - xmpp:feedback@shakespeare.lit
        -
          modules:
            - mod_disco
            - mod_vcard
          name: admin-addresses
          urls:
            - mailto:xmpp@shakespeare.lit
            - xmpp:admins@shakespeare.lit

## mod_fail2ban

The module bans IPs that show the malicious signs. Currently only C2S authentication failures are detected.

Unlike the standalone program, mod_fail2ban clears the record of authentication failures after some time since the first failure or on a successful authentication. It also does not simply block network traffic, but provides the client with a descriptive error message.

> Warning

> You should not use this module behind a proxy or load balancer. ejabberd will see the failures as coming from the load balancer and, when the threshold of auth failures is reached, will reject all connections coming from the load balancer. You can lock all your user base out of ejabberd when using this module behind a proxy.

Available options:

- access: AccessName
  Specify an access rule for whitelisting IP addresses or networks. If the rule returns allow for a given IP address, that address will never be banned. The AccessName should be of type ip. The default value is none.

- c2s_auth_ban_lifetime: timeout()
  The lifetime of the IP ban caused by too many C2S authentication failures. The default value is 1 hour.

- c2s_max_auth_failures: Number
  The number of C2S authentication failures to trigger the IP ban. The default value is 20.

## mod_host_meta

added in 22.05

This module serves small host-meta files as described in XEP-0156: Discovering Alternative XMPP Connection Methods.

To use this module, in addition to adding it to the modules section, you must also enable it in listen → ejabberd_http → request_handlers.

Notice it only works if ejabberd_http has tls enabled.

Available options:

- bosh_service_url: undefined | auto | BoshURL
  BOSH service URL to announce. The keyword @HOST@ is replaced with the real virtual host name. If set to auto, it will build the URL of the first configured BOSH request handler. The default value is auto.

- websocket_url: undefined | auto | WebSocketURL
  WebSocket URL to announce. The keyword @HOST@ is replaced with the real virtual host name. If set to auto, it will build the URL of the first configured WebSocket request handler. The default value is auto.

Example:

    listen:
      -
        port: 443
        module: ejabberd_http
        tls: true
        request_handlers:
          /bosh: mod_bosh
          /ws: ejabberd_http_ws
          /.well-known/host-meta: mod_host_meta
          /.well-known/host-meta.json: mod_host_meta

    modules:
      mod_bosh: {}
      mod_host_meta:
        bosh_service_url: "https://@HOST@:5443/bosh"
        websocket_url: "wss://@HOST@:5443/ws"

## mod_http_api

This module provides a ReST interface to call ejabberd API commands using JSON data.

To use this module, in addition to adding it to the modules section, you must also enable it in listen → ejabberd_http → request_handlers.

To use a specific API version N, when defining the URL path in the request_handlers, add a vN. For example: /api/v2: mod_http_api

To run a command, send a POST request to the corresponding URL: http://localhost:5280/api/<command_name>

The module has no options.

Example:

    listen:
      -
        port: 5280
        module: ejabberd_http
        request_handlers:
          /api: mod_http_api

    modules:
      mod_http_api: {}

## mod_http_fileserver

This simple module serves files from the local disk over HTTP.

Available options:

- accesslog: Path
  File to log accesses using an Apache-like format. No log will be recorded if this option is not specified.

- content_types: {Extension: Type}
  Specify mappings of extension to content type. There are several content types already defined. With this option you can add new definitions or modify existing ones. The default values are:

  Example:

      content_types:
        .css: text/css
        .gif: image/gif
        .html: text/html
        .jar: application/java-archive
        .jpeg: image/jpeg
        .jpg: image/jpeg
        .js: text/javascript
        .png: image/png
        .svg: image/svg+xml
        .txt: text/plain
        .xml: application/xml
        .xpi: application/x-xpinstall
        .xul: application/vnd.mozilla.xul+xml

- custom_headers: {Name: Value}
  Indicate custom HTTP headers to be included in all responses. There are no custom headers by default.

- default_content_type: Type
  Specify the content type to use for unknown extensions. The default value is application/octet-stream.

- directory_indices: [Index, ...]
  Indicate one or more directory index files, similarly to Apache’s DirectoryIndex variable. When an HTTP request hits a directory instead of a regular file, those directory indices are looked in order, and the first one found is returned. The default value is an empty list.

- docroot: Path
  Directory to serve the files from. This is a mandatory option.

- must_authenticate_with: [{Username, Hostname}, ...]
  List of accounts that are allowed to use this service. Default value: [].

Examples:

This example configuration will serve the files from the local directory /var/www in the address http://example.org:5280/pub/content/. In this example a new content type ogg is defined, png is redefined, and jpg definition is deleted:

    listen:
      -
        port: 5280
        module: ejabberd_http
        request_handlers:
          /pub/content: mod_http_fileserver

    modules:
      mod_http_fileserver:
        docroot: /var/www
        accesslog: /var/log/ejabberd/access.log
        directory_indices:
          - index.html
          - main.htm
        custom_headers:
          X-Powered-By: Erlang/OTP
          X-Fry: "It's a widely-believed fact!"
        content_types:
          .ogg: audio/ogg
          .png: image/png
        default_content_type: text/html

## mod_http_upload

This module allows for requesting permissions to upload a file via HTTP as described in XEP-0363: HTTP File Upload. If the request is accepted, the client receives a URL for uploading the file and another URL from which that file can later be downloaded.

In order to use this module, it must be enabled in listen → ejabberd_http → request_handlers.

Available options:

- access: AccessName
  This option defines the access rule to limit who is permitted to use the HTTP upload service. The default value is local. If no access rule of that name exists, no user will be allowed to use the service.

- custom_headers: {Name: Value}
  This option specifies additional header fields to be included in all HTTP responses. By default no custom headers are included.

- dir_mode: Permission
  This option defines the permission bits of the docroot directory and any directories created during file uploads. The bits are specified as an octal number (see the chmod(1) manual page) within double quotes. For example: "0755". The default is undefined, which means no explicit permissions will be set.

- docroot: Path
  Uploaded files are stored below the directory specified (as an absolute path) with this option. The keyword @HOME@ is replaced with the home directory of the user running ejabberd, and the keyword @HOST@ with the virtual host name. The default value is "@HOME@/upload".

- external_secret: Text
  This option makes it possible to offload all HTTP Upload processing to a separate HTTP server. Both ejabberd and the HTTP server should share this secret and behave exactly as described at Prosody’s mod_http_upload_external in the Implementation section. There is no default value.

- file_mode: Permission
  This option defines the permission bits of uploaded files. The bits are specified as an octal number (see the chmod(1) manual page) within double quotes. For example: "0644". The default is undefined, which means no explicit permissions will be set.

- get_url: URL
  This option specifies the initial part of the GET URLs used for downloading the files. The default value is undefined. When this option is undefined, this option is set to the same value as put_url. The keyword @HOST@ is replaced with the virtual host name. NOTE: if GET requests are handled by mod_http_upload, the get_url must match the put_url. Setting it to a different value only makes sense if an external web server or mod_http_fileserver is used to serve the uploaded files.

- host
  Deprecated. Use hosts instead.

- hosts: [Host, ...]
  This option defines the Jabber IDs of the service. If the hosts option is not specified, the only Jabber ID will be the hostname of the virtual host with the prefix "upload.". The keyword @HOST@ is replaced with the real virtual host name.

- jid_in_url: node | sha1
  When this option is set to node, the node identifier of the user’s JID (i.e., the user name) is included in the GET and PUT URLs generated by mod_http_upload. Otherwise, a SHA-1 hash of the user’s bare JID is included instead. The default value is sha1.

- max_size: Size
  This option limits the acceptable file size. Either a number of bytes (larger than zero) or infinity must be specified. The default value is 104857600.

- name: Name
  A name of the service in the Service Discovery. This will only be displayed by special XMPP clients. The default value is "HTTP File Upload".

- put_url: URL
  This option specifies the initial part of the PUT URLs used for file uploads. The keyword @HOST@ is replaced with the virtual host name. NOTE: different virtual hosts cannot use the same PUT URL. The default value is "https://@HOST@:5443/upload".

- rm_on_unregister: true | false
  This option specifies whether files uploaded by a user should be removed when that user is unregistered. The default value is true.

- secret_length: Length
  This option defines the length of the random string included in the GET and PUT URLs generated by mod_http_upload. The minimum length is 8 characters, but it is recommended to choose a larger value. The default value is 40.

- service_url
  Deprecated.

- thumbnail: true | false
  This option specifies whether ejabberd should create thumbnails of uploaded images. If a thumbnail is created, a <thumbnail/> element that contains the download <uri/> and some metadata is returned with the PUT response. The default value is false.

- vcard: vCard
  A custom vCard of the service that will be displayed by some XMPP clients in Service Discovery. The value of vCard is a YAML map constructed from an XML representation of vCard. Since the representation has no attributes, the mapping is straightforward.

  Example:

      # This XML representation of vCard:
      #   <vCard xmlns='vcard-temp'>
      #     <FN>Conferences</FN>
      #     <ADR>
      #       <WORK/>
      #       <STREET>Elm Street</STREET>
      #     </ADR>
      #   </vCard>
      #
      # is translated to:
      vcard:
        fn: Conferences
        adr:
          -
            work: true
            street: Elm Street

Example:

    listen:
      -
        port: 5443
        module: ejabberd_http
        tls: true
        request_handlers:
          /upload: mod_http_upload

    modules:
      mod_http_upload:
        docroot: /ejabberd/upload
        put_url: "https://@HOST@:5443/upload"

## mod_http_upload_quota

This module adds quota support for mod_http_upload.

This module depends on mod_http_upload.

Available options:

- access_hard_quota: AccessName
  This option defines which access rule is used to specify the "hard quota" for the matching JIDs. That rule must yield a positive number for any JID that is supposed to have a quota limit. This is the number of megabytes a corresponding user may upload. When this threshold is exceeded, ejabberd deletes the oldest files uploaded by that user until their disk usage equals or falls below the specified soft quota (see access_soft_quota). The default value is hard_upload_quota.

- access_soft_quota: AccessName
  This option defines which access rule is used to specify the "soft quota" for the matching JIDs. That rule must yield a positive number of megabytes for any JID that is supposed to have a quota limit. See the description of the access_hard_quota option for details. The default value is soft_upload_quota.

- max_days: Days
  If a number larger than zero is specified, any files (and directories) older than this number of days are removed from the subdirectories of the docroot directory, once per day. The default value is infinity.

Examples:

Please note that it’s not necessary to specify the access_hard_quota and access_soft_quota options in order to use the quota feature. You can stick to the default names and just specify access rules such as those in this example:

    shaper_rules:
      soft_upload_quota:
        1000: all # MiB
      hard_upload_quota:
        1100: all # MiB

    modules:
      mod_http_upload: {}
      mod_http_upload_quota:
        max_days: 100

## mod_jidprep

This module allows XMPP clients to ask the server to normalize a JID as per the rules specified in RFC 6122: XMPP Address Format. This might be useful for clients in certain constrained environments, or for testing purposes.

Available options:

- access: AccessName
  This option defines which access rule will be used to control who is allowed to use this service. The default value is local.

## mod_last

This module adds support for XEP-0012: Last Activity. It can be used to discover when a disconnected user last accessed the server, to know when a connected user was last active on the server, or to query the uptime of the ejabberd server.

Available options:

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

## mod_legacy_auth

The module implements XEP-0078: Non-SASL Authentication.

> Note

> This type of authentication was obsoleted in 2008 and you unlikely need this module unless you have something like outdated Jabber bots.

The module has no options.

## mod_mam

This module implements XEP-0313: Message Archive Management and XEP-0441: Message Archive Management Preferences. Compatible XMPP clients can use it to store their chat history on the server.

Available options:

- access_preferences: AccessName
  This access rule defines who is allowed to modify the MAM preferences. The default value is all.

- assume_mam_usage: true | false
  This option determines how ejabberd’s stream management code (see mod_stream_mgmt) handles unacknowledged messages when the connection is lost. Usually, such messages are either bounced or resent. However, neither is done for messages that were stored in the user’s MAM archive if this option is set to true. In this case, ejabberd assumes those messages will be retrieved from the archive. The default value is false.

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- clear_archive_on_room_destroy: true | false
  Whether to destroy message archive of a room (see mod_muc) when it gets destroyed. The default value is true.

- compress_xml: true | false
  When enabled, new messages added to archives are compressed using a custom compression algorithm. This feature works only with SQL backends. The default value is false.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- default: always | never | roster
  The option defines default policy for chat history. When always is set every chat message is stored. With roster only chat history with contacts from user’s roster is stored. And never fully disables chat history. Note that a client can change its policy via protocol commands. The default value is never.

- request_activates_archiving: true | false
  If the value is true, no messages are stored for a user until their client issue a MAM request, regardless of the value of the default option. Once the server received a request, that user’s messages are archived as usual. The default value is false.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

- user_mucsub_from_muc_archive: true | false
  When this option is disabled, for each individual subscriber a separate mucsub message is stored. With this option enabled, when a user fetches archive virtual mucsub, messages are generated from muc archives. The default value is false.

## mod_matrix_gw

added in 24.02

Matrix gateway.

Available options:

- host: Host
  This option defines the Jabber IDs of the service. If the host option is not specified, the Jabber ID will be the hostname of the virtual host with the prefix "matrix.". The keyword @HOST@ is replaced with the real virtual host name.

- key: string()
  Value of the matrix signing key, in base64.

- key_name: string()
  Name of the matrix signing key.

- matrix_domain: Domain
  Specify a domain in the Matrix federation. The keyword @HOST@ is replaced with the hostname. The default value is @HOST@.

- matrix_id_as_jid: true | false
  If set to true, all packets failing to be delivered via an XMPP server-to-server connection will then be routed to the Matrix gateway by translating a Jabber ID user@matrixdomain.tld to a Matrix user identifier @user:matrixdomain.tld. When set to false, messages must be explicitly sent to the matrix gateway service Jabber ID to be routed to a remote Matrix server. In this case, to send a message to Matrix user @user:matrixdomain.tld, the client must send a message to the JID user%matrixdomain.tld@matrix.myxmppdomain.tld, where matrix.myxmppdomain.tld is the JID of the gateway service as set by the host option. The default is false.

Example:

    listen:
      -
        port: 8448
        module: ejabberd_http
        tls: true
        request_handlers:
          "/_matrix": mod_matrix_gw

    modules:
      mod_matrix_gw:
        key_name: "key1"
        key: "XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXX"
        matrix_id_as_jid: true

## mod_metrics

This module sends events to external backend (by now only grapherl is supported). Supported events are:

- sm_register_connection

- sm_remove_connection

- user_send_packet

- user_receive_packet

- s2s_send_packet

- s2s_receive_packet

- register_user

- remove_user

- offline_message

When enabled, every call to these hooks triggers a counter event to be sent to the external backend.

Available options:

- ip: IPv4Address
  IPv4 address where the backend is located. The default value is 127.0.0.1.

- port: Port
  An internet port number at which the backend is listening for incoming connections/packets. The default value is 11111.

## mod_mix

added in 16.03 and improved in 19.02

This module is an experimental implementation of XEP-0369: Mediated Information eXchange (MIX). It’s asserted that the MIX protocol is going to replace the MUC protocol in the future (see mod_muc).

To learn more about how to use that feature, you can refer to our tutorial: Getting started with MIX

The module depends on mod_mam.

Available options:

- access_create: AccessName
  An access rule to control MIX channels creations. The default value is all.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- host
  Deprecated. Use hosts instead.

- hosts: [Host, ...]
  This option defines the Jabber IDs of the service. If the hosts option is not specified, the only Jabber ID will be the hostname of the virtual host with the prefix "mix.". The keyword @HOST@ is replaced with the real virtual host name.

- name: Name
  A name of the service in the Service Discovery. This will only be displayed by special XMPP clients. The default value is Channels.

## mod_mix_pam

This module implements XEP-0405: Mediated Information eXchange (MIX): Participant Server Requirements. The module is needed if MIX compatible clients on your server are going to join MIX channels (either on your server or on any remote servers).

> Note

> mod_mix is not required for this module to work, however, without mod_mix_pam the MIX functionality of your local XMPP clients will be impaired.

Available options:

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

## mod_mqtt

This module adds support for the MQTT protocol version 3.1.1 and 5.0. Remember to configure mod_mqtt in modules and listen sections.

Available options:

- access_publish: {TopicFilter: AccessName}
  Access rules to restrict access to topics for publishers. By default there are no restrictions.

- access_subscribe: {TopicFilter: AccessName}
  Access rules to restrict access to topics for subscribers. By default there are no restrictions.

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- match_retained_limit: pos_integer() | infinity
  The option limits the number of retained messages returned to a client when it subscribes to some topic filter. The default value is 1000.

- max_queue: Size
  Maximum queue size for outgoing packets. The default value is 5000.

- max_topic_aliases: 0..65535
  The maximum number of aliases a client is able to associate with the topics. The default value is 100.

- max_topic_depth: Depth
  The maximum topic depth, i.e. the number of slashes (/) in the topic. The default value is 8.

- queue_type: ram | file
  Same as top-level queue_type option, but applied to this module only.

- ram_db_type: mnesia
  Same as top-level default_ram_db option, but applied to this module only.

- session_expiry: timeout()
  The option specifies how long to wait for an MQTT session resumption. When 0 is set, the session gets destroyed when the underlying client connection is closed. The default value is 5 minutes.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

## mod_mqtt_bridge

This module adds ability to synchronize local MQTT topics with data on remote servers It can update topics on remote servers when local user updates local topic, or can subscribe for changes on remote server, and update local copy when remote data is updated. It is available since ejabberd 23.01.

Available options:

- replication_user: JID
  Identifier of a user that will be assigned as owner of local changes.

- servers: {ServerUrl: {publish: [TopicPairs, subscribe: [TopicPairs], authentication: [AuthInfo]}}]
  Declaration of data to share, must contain publish or subscribe or both, and authentication section with username/password field or certfile pointing to client certificate. Accepted urls can use schema mqtt, mqtts (mqtt with tls), mqtt5, mqtt5s (both to trigger v5 protocol), ws, wss, ws5, wss5. Certificate authentication can be only used with mqtts, mqtt5s, wss, wss5.

Example:

    modules:
      mod_mqtt_bridge:
        servers:
          "mqtt://server.com":
            publish:
              "localA": "remoteA" # local changes to 'localA' will be replicated on remote server as 'remoteA'
              "topicB": "topicB"
            subscribe:
              "remoteB": "localB" # changes to 'remoteB' on remote server will be stored as 'localB' on local server
            authentication:
              certfile: "/etc/ejabberd/mqtt_server.pem"
        replication_user: "mqtt@xmpp.server.com"

## mod_muc

This module provides support for XEP-0045: Multi-User Chat. Users can discover existing rooms, join or create them. Occupants of a room can chat in public or have private chats.

The MUC service allows any Jabber ID to register a nickname, so nobody else can use that nickname in any room in the MUC service. To register a nickname, open the Service Discovery in your XMPP client and register in the MUC service.

It is also possible to register a nickname in a room, so nobody else can use that nickname in that room. If a nick is registered in the MUC service, that nick cannot be registered in any room, and vice versa: a nick that is registered in a room cannot be registered at the MUC service.

This module supports clustering and load balancing. One module can be started per cluster node. Rooms are distributed at creation time on all available MUC module instances. The multi-user chat module is clustered but the rooms themselves are not clustered nor fault-tolerant: if the node managing a set of rooms goes down, the rooms disappear and they will be recreated on an available node on first connection attempt.

Available options:

- access: AccessName
  You can specify who is allowed to use the Multi-User Chat service. By default everyone is allowed to use it.

- access_admin: AccessName
  This option specifies who is allowed to administrate the Multi-User Chat service. The default value is none, which means that only the room creator can administer their room. The administrators can send a normal message to the service JID, and it will be shown in all active rooms as a service message. The administrators can send a groupchat message to the JID of an active room, and the message will be shown in the room as a service message.

- access_create: AccessName
  To configure who is allowed to create new rooms at the Multi-User Chat service, this option can be used. The default value is all, which means everyone is allowed to create rooms.

- access_mam: AccessName
  To configure who is allowed to modify the mam room option. The default value is all, which means everyone is allowed to modify that option.

- access_persistent: AccessName
  To configure who is allowed to modify the persistent room option. The default value is all, which means everyone is allowed to modify that option.

- access_register: AccessName
  improved in 23.10 This option specifies who is allowed to register nickname within the Multi-User Chat service and rooms. The default is all for backward compatibility, which means that any user is allowed to register any free nick in the MUC service and in the rooms.

- cleanup_affiliations_on_start: true | false
  added in 22.05 Remove affiliations for non-existing local users on startup. The default value is false.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- default_room_options: Options
  Define the default room options. Note that the creator of a room can modify the options of his room at any time using an XMPP client with MUC capability. The Options are:

  - allow_change_subj: true | false
    Allow occupants to change the subject. The default value is true.

  - allow_private_messages_from_visitors: anyone | moderators | nobody Visitors can send private messages to other occupants. The default value is anyone which means visitors can send private messages to any occupant.

  - allow_query_users: true | false
    Occupants can send IQ queries to other occupants. The default value is true.

  - allow_subscription: true | false
    Allow users to subscribe to room events as described in Multi-User Chat Subscriptions. The default value is false.

  - allow_user_invites: true | false
    Allow occupants to send invitations. The default value is false.

  - allow_visitor_nickchange: true | false
    Allow visitors to change nickname. The default value is true.

  - allow_visitor_status: true | false
    Allow visitors to send status text in presence updates. If disallowed, the status text is stripped before broadcasting the presence update to all the room occupants. The default value is true.

  - allow_voice_requests: true | false
    Allow visitors in a moderated room to request voice. The default value is true.

  - allowpm: anyone | participants | moderators | none
    Who can send private messages. The default value is anyone.

  - anonymous: true | false
    The room is anonymous: occupants don’t see the real JIDs of other occupants. Note that the room moderators can always see the real JIDs of the occupants. The default value is true.

  - captcha_protected: true | false
    When a user tries to join a room where they have no affiliation (not owner, admin or member), the room requires them to fill a CAPTCHA challenge (see section CAPTCHA in order to accept their join in the room. The default value is false.

  - description: Room Description
    Short description of the room. The default value is an empty string.

  - enable_hats: true | false
    Allow extended roles as defined in XEP-0317 Hats. The default value is false.

  - lang: Language
    Preferred language for the discussions in the room. The language format should conform to RFC 5646. There is no value by default.

  - logging: true | false
    The public messages are logged using mod_muc_log. The default value is false.

  - mam: true | false
    Enable message archiving. Implies mod_mam is enabled. The default value is false.

  - max_users: Number
    Maximum number of occupants in the room. The default value is 200.

  - members_by_default: true | false
    The occupants that enter the room are participants by default, so they have "voice". The default value is true.

  - members_only: true | false
    Only members of the room can enter. The default value is false.

  - moderated: true | false
    Only occupants with "voice" can send public messages. The default value is true.

  - password: Password
    Password of the room. Implies option password_protected set to true. There is no default value.

  - password_protected: true | false
    The password is required to enter the room. The default value is false.

  - persistent: true | false
    The room persists even if the last participant leaves. The default value is false.

  - presence_broadcast: [moderator | participant | visitor, ...] List of roles for which presence is broadcasted. The list can contain one or several of: moderator, participant, visitor. The default value is shown in the example below:

    Example:

        presence_broadcast:
          - moderator
          - participant
          - visitor

  - public: true | false
    The room is public in the list of the MUC service, so it can be discovered. MUC admins and room participants will see private rooms in Service Discovery if their XMPP client supports this feature. The default value is true.

  - public_list: true | false
    The list of participants is public, without requiring to enter the room. The default value is true.

  - pubsub: PubSub Node
    XMPP URI of associated Publish/Subscribe node. The default value is an empty string.

  - title: Room Title
    A human-readable title of the room. There is no default value

  - vcard: vCard
    A custom vCard for the room. See the equivalent mod_muc option.The default value is an empty string.

  - voice_request_min_interval: Number
    Minimum interval between voice requests, in seconds. The default value is 1800.

- hibernation_timeout: infinity | Seconds
  Timeout before hibernating the room process, expressed in seconds. The default value is infinity.

- history_size: Size
  A small history of the current discussion is sent to users when they enter the room. With this option you can define the number of history messages to keep and send to users joining the room. The value is a non-negative integer. Setting the value to 0 disables the history feature and, as a result, nothing is kept in memory. The default value is 20. This value affects all rooms on the service. NOTE: modern XMPP clients rely on Message Archives (XEP-0313), so feel free to disable the history feature if you’re only using modern clients and have mod_mam module loaded.

- host
  Deprecated. Use hosts instead.

- hosts: [Host, ...]
  This option defines the Jabber IDs of the service. If the hosts option is not specified, the only Jabber ID will be the hostname of the virtual host with the prefix "conference.". The keyword @HOST@ is replaced with the real virtual host name.

- max_captcha_whitelist: Number
  added in 21.01 This option defines the maximum number of characters that Captcha Whitelist can have when configuring the room. The default value is infinity.

- max_password: Number
  added in 21.01 This option defines the maximum number of characters that Password can have when configuring the room. The default value is infinity.

- max_room_desc: Number
  This option defines the maximum number of characters that Room Description can have when configuring the room. The default value is infinity.

- max_room_id: Number
  This option defines the maximum number of characters that Room ID can have when creating a new room. The default value is infinity.

- max_room_name: Number
  This option defines the maximum number of characters that Room Name can have when configuring the room. The default value is infinity.

- max_rooms_discoitems: Number
  When there are more rooms than this Number, only the non-empty ones are returned in a Service Discovery query. The default value is 100.

- max_user_conferences: Number
  This option defines the maximum number of rooms that any given user can join. The default value is 100. This option is used to prevent possible abuses. Note that this is a soft limit: some users can sometimes join more conferences in cluster configurations.

- max_users: Number
  This option defines at the service level, the maximum number of users allowed per room. It can be lowered in each room configuration but cannot be increased in individual room configuration. The default value is 200.

- max_users_admin_threshold: Number
  This option defines the number of service admins or room owners allowed to enter the room when the maximum number of allowed occupants was reached. The default limit is 5.

- max_users_presence: Number
  This option defines after how many users in the room, it is considered overcrowded. When a MUC room is considered overcrowded, presence broadcasts are limited to reduce load, traffic and excessive presence "storm" received by participants. The default value is 1000.

- min_message_interval: Number
  This option defines the minimum interval between two messages send by an occupant in seconds. This option is global and valid for all rooms. A decimal value can be used. When this option is not defined, message rate is not limited. This feature can be used to protect a MUC service from occupant abuses and limit number of messages that will be broadcasted by the service. A good value for this minimum message interval is 0.4 second. If an occupant tries to send messages faster, an error is send back explaining that the message has been discarded and describing the reason why the message is not acceptable.

- min_presence_interval: Number
  This option defines the minimum of time between presence changes coming from a given occupant in seconds. This option is global and valid for all rooms. A decimal value can be used. When this option is not defined, no restriction is applied. This option can be used to protect a MUC service for occupants abuses. If an occupant tries to change its presence more often than the specified interval, the presence is cached by ejabberd and only the last presence is broadcasted to all occupants in the room after expiration of the interval delay. Intermediate presence packets are silently discarded. A good value for this option is 4 seconds.

- name: string()
  The value of the service name. This name is only visible in some clients that support XEP-0030: Service Discovery. The default is Chatrooms.

- preload_rooms: true | false
  Whether to load all persistent rooms in memory on startup. If disabled, the room is only loaded on first participant join. The default is true. It makes sense to disable room preloading when the number of rooms is high: this will improve server startup time and memory consumption.

- queue_type: ram | file
  Same as top-level queue_type option, but applied to this module only.

- ram_db_type: mnesia | sql
  Same as top-level default_ram_db option, but applied to this module only.

- regexp_room_id: string()
  This option defines the regular expression that a Room ID must satisfy to allow the room creation. The default value is the empty string.

- room_shaper: none | ShaperName
  This option defines shaper for the MUC rooms. The default value is none.

- user_message_shaper: none | ShaperName
  This option defines shaper for the users messages. The default value is none.

- user_presence_shaper: none | ShaperName
  This option defines shaper for the users presences. The default value is none.

- vcard: vCard
  A custom vCard of the service that will be displayed by some XMPP clients in Service Discovery. The value of vCard is a YAML map constructed from an XML representation of vCard. Since the representation has no attributes, the mapping is straightforward.

  Example:

      # This XML representation of vCard:
      #   <vCard xmlns='vcard-temp'>
      #     <FN>Conferences</FN>
      #     <ADR>
      #       <WORK/>
      #       <STREET>Elm Street</STREET>
      #     </ADR>
      #   </vCard>
      #
      # is translated to:
      vcard:
        fn: Conferences
        adr:
          -
            work: true
            street: Elm Street

## mod_muc_admin

This module provides commands to administer local MUC services and their MUC rooms. It also provides simple WebAdmin pages to view the existing rooms.

This module depends on mod_muc.

Available options:

- subscribe_room_many_max_users: Number
  added in 22.05 How many users can be subscribed to a room at once using the subscribe_room_many command. The default value is 50.

## mod_muc_log

This module enables optional logging of Multi-User Chat (MUC) public conversations to HTML. Once you enable this module, users can join a room using a MUC capable XMPP client, and if they have enough privileges, they can request the configuration form in which they can set the option to enable room logging.

Features:

- Room details are added on top of each page: room title, JID, author, subject and configuration.

- The room JID in the generated HTML is a link to join the room (using XMPP URI).

- Subject and room configuration changes are tracked and displayed.

- Joins, leaves, nick changes, kicks, bans and /me are tracked and displayed, including the reason if available.

- Generated HTML files are XHTML 1.0 Transitional and CSS compliant.

- Timestamps are self-referencing links.

- Links on top for quicker navigation: Previous day, Next day, Up.

- CSS is used for style definition, and a custom CSS file can be used.

- URLs on messages and subjects are converted to hyperlinks.

- Timezone used on timestamps is shown on the log files.

- A custom link can be added on top of each page.

The module depends on mod_muc.

Available options:

- access_log: AccessName
  This option restricts which occupants are allowed to enable or disable room logging. The default value is muc_admin. NOTE: for this default setting you need to have an access rule for muc_admin in order to take effect.

- cssfile: Path | URL
  With this option you can set whether the HTML files should have a custom CSS file or if they need to use the embedded CSS. Allowed values are either Path to local file or an URL to a remote file. By default a predefined CSS will be embedded into the HTML page.

- dirname: room_jid | room_name
  Configure the name of the room directory. If set to room_jid, the room directory name will be the full room JID. Otherwise, the room directory name will be only the room name, not including the MUC service name. The default value is room_jid.

- dirtype: subdirs | plain
  The type of the created directories can be specified with this option. If set to subdirs, subdirectories are created for each year and month. Otherwise, the names of the log files contain the full date, and there are no subdirectories. The default value is subdirs.

- file_format: html | plaintext
  Define the format of the log files: html stores in HTML format, plaintext stores in plain text. The default value is html.

- file_permissions: {mode: Mode, group: Group}
  Define the permissions that must be used when creating the log files: the number of the mode, and the numeric id of the group that will own the files. The default value is shown in the example below:

  Example:

      file_permissions:
        mode: 644
        group: 33

- outdir: Path
  This option sets the full path to the directory in which the HTML files should be stored. Make sure the ejabberd daemon user has write access on that directory. The default value is www/muc.

- spam_prevention: true | false
  If set to true, a special attribute is added to links that prevent their indexation by search engines. The default value is true, which mean that nofollow attributes will be added to user submitted links.

- timezone: local | universal
  The time zone for the logs is configurable with this option. If set to local, the local time, as reported to Erlang emulator by the operating system, will be used. Otherwise, UTC time will be used. The default value is local.

- top_link: {URL: Text}
  With this option you can customize the link on the top right corner of each log file. The default value is shown in the example below:

  Example:

      top_link:
        /: Home

- url: URL
  A top level URL where a client can access logs of a particular conference. The conference name is appended to the URL if dirname option is set to room_name or a conference JID is appended to the URL otherwise. There is no default value.

## mod_muc_occupantid

added in 23.10

This module implements XEP-0421: Anonymous unique occupant identifiers for MUCs.

When the module is enabled, the feature is enabled in all semi-anonymous rooms.

The module has no options.

## mod_muc_rtbl

added in 23.04

This module implement Real-time blocklists for MUC rooms.

It works by observing remote pubsub node conforming with specification described in https://xmppbl.org/.

Available options:

- rtbl_node: PubsubNodeName
  Name of pubsub node that should be used to track blocked users. The default value is muc_bans_sha256.

- rtbl_server: Domain
  Domain of xmpp server that serves block list. The default value is xmppbl.org

## mod_multicast

This module implements a service for XEP-0033: Extended Stanza Addressing.

Available options:

- access: Access
  The access rule to restrict who can send packets to the multicast service. Default value: all.

- host
  Deprecated. Use hosts instead.

- hosts: [Host, ...]
  This option defines the Jabber IDs of the service. If the hosts option is not specified, the only Jabber ID will be the hostname of the virtual host with the prefix "multicast.". The keyword @HOST@ is replaced with the real virtual host name. The default value is multicast.@HOST@.

- limits: Sender: Stanza: Number
  Specify a list of custom limits which override the default ones defined in XEP-0033. Limits are defined per sender type and stanza type, where:

  - sender can be: local or remote.

  - stanza can be: message or presence.

  - number can be a positive integer or infinite.

    Example:

        # Default values:
        local:
          message: 100
          presence: 100
        remote:
          message: 20
          presence: 20

- name
  Service name to provide in the Info query to the Service Discovery. Default is "Multicast".

- vcard
  vCard element to return when queried. Default value is undefined.

Example:

    # Only admins can send packets to multicast service
    access_rules:
      multicast:
        - allow: admin

    # If you want to allow all your users:
    access_rules:
      multicast:
        - allow

    # This allows both admins and remote users to send packets,
    # but does not allow local users
    acl:
      allservers:
        server_glob: "*"
    access_rules:
      multicast:
        - allow: admin
        - deny: local
        - allow: allservers

    modules:
      mod_multicast:
         host: multicast.example.org
         access: multicast
         limits:
           local:
             message: 40
             presence: infinite
           remote:
             message: 150

## mod_offline

This module implements XEP-0160: Best Practices for Handling Offline Messages and XEP-0013: Flexible Offline Message Retrieval. This means that all messages sent to an offline user will be stored on the server until that user comes online again. Thus it is very similar to how email works. A user is considered offline if no session presence priority > 0 are currently open.

> Note

> ejabberdctl has a command to delete expired messages (see chapter Managing an ejabberd server in online documentation.

Available options:

- access_max_user_messages: AccessName
  This option defines which access rule will be enforced to limit the maximum number of offline messages that a user can have (quota). When a user has too many offline messages, any new messages that they receive are discarded, and a <resource-constraint/> error is returned to the sender. The default value is max_user_offline_messages.

- bounce_groupchat: true | false
  This option is use the disable an optimization that avoids bouncing error messages when groupchat messages could not be stored as offline. It will reduce chat room load, without any drawback in standard use cases. You may change default value only if you have a custom module which uses offline hook after mod_offline. This option can be useful for both standard MUC and MucSub, but the bounce is much more likely to happen in the context of MucSub, so it is even more important to have it on large MucSub services. The default value is false, meaning the optimization is enabled.

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- store_empty_body: true | false | unless_chat_state
  Whether or not to store messages that lack a <body/> element. The default value is unless_chat_state, which tells ejabberd to store messages even if they lack the <body/> element, unless they only contain a chat state notification (as defined in XEP-0085: Chat State Notifications.

- store_groupchat: true | false
  Whether or not to store groupchat messages. The default value is false.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

- use_mam_for_storage: true | false
  This is an experimental option. Enabling this option, mod_offline uses the mod_mam archive table instead of its own spool table to retrieve the messages received when the user was offline. This allows client developers to slowly drop XEP-0160 and rely on XEP-0313 instead. It also further reduces the storage required when you enable MucSub. Enabling this option has a known drawback for the moment: most of flexible message retrieval queries don’t work (those that allow retrieval/deletion of messages by id), but this specification is not widely used. The default value is false to keep former behaviour as default.

Examples:

This example allows power users to have as much as 5000 offline messages, administrators up to 2000, and all the other users up to 100:

    acl:
      admin:
        user:
          - admin1@localhost
          - admin2@example.org
      poweruser:
        user:
          - bob@example.org
          - jane@example.org

    shaper_rules:
      max_user_offline_messages:
        - 5000: poweruser
        - 2000: admin
        - 100

    modules:
      ...
      mod_offline:
        access_max_user_messages: max_user_offline_messages
      ...

## mod_ping

This module implements support for XEP-0199: XMPP Ping and periodic keepalives. When this module is enabled ejabberd responds correctly to ping requests, as defined by the protocol.

Available options:

- ping_ack_timeout: timeout()
  How long to wait before deeming that a client has not answered a given server ping request. NOTE: when mod_stream_mgmt is loaded and stream management is enabled by a client, this value is ignored, and the `ack_timeout` applies instead. The default value is undefined.

- ping_interval: timeout()
  How often to send pings to connected clients, if option send_pings is set to true. If a client connection does not send or receive any stanza within this interval, a ping request is sent to the client. The default value is 1 minute.

- send_pings: true | false
  If this option is set to true, the server sends pings to connected clients that are not active in a given interval defined in ping_interval option. This is useful to keep client connections alive or checking availability. The default value is false.

- timeout_action: none | kill
  What to do when a client does not answer to a server ping request in less than period defined in ping_ack_timeout option: kill means destroying the underlying connection, none means to do nothing. NOTE: when mod_stream_mgmt is loaded and stream management is enabled by a client, killing the client connection doesn’t mean killing the client session - the session will be kept alive in order to give the client a chance to resume it. The default value is none.

Example:

    modules:
      mod_ping:
        send_pings: true
        ping_interval: 4 min
        timeout_action: kill

## mod_pres_counter

This module detects flood/spam in presence subscriptions traffic. If a user sends or receives more of those stanzas in a given time interval, the exceeding stanzas are silently dropped, and a warning is logged.

Available options:

- count: Number
  The number of subscription presence stanzas (subscribe, unsubscribe, subscribed, unsubscribed) allowed for any direction (input or output) per time defined in interval option. Please note that two users subscribing to each other usually generate 4 stanzas, so the recommended value is 4 or more. The default value is 5.

- interval: timeout()
  The time interval. The default value is 1 minute.

Example:

    modules:
      mod_pres_counter:
        count: 5
        interval: 30 secs

## mod_privacy

This module implements XEP-0016: Privacy Lists.

> Note

> Nowadays modern XMPP clients rely on XEP-0191: Blocking Command which is implemented by mod_blocking module. However, you still need mod_privacy loaded in order for mod_blocking to work.

Available options:

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

## mod_private

This module adds support for XEP-0049: Private XML Storage.

Using this method, XMPP entities can store private data on the server, retrieve it whenever necessary and share it between multiple connected clients of the same user. The data stored might be anything, as long as it is a valid XML. One typical usage is storing a bookmark of all user’s conferences (XEP-0048: Bookmarks).

It also implements the bookmark conversion described in XEP-0402: PEP Native Bookmarks, see the command bookmarks_to_pep API.

Available options:

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

## mod_privilege

This module is an implementation of XEP-0356: Privileged Entity. This extension allows components to have privileged access to other entity data (send messages on behalf of the server or on behalf of a user, get/set user roster, access presence information, etc.). This may be used to write powerful external components, for example implementing an external PEP or MAM service.

By default a component does not have any privileged access. It is worth noting that the permissions grant access to the component to a specific data type for all users of the virtual host on which mod_privilege is loaded.

Make sure you have a listener configured to connect your component. Check the section about listening ports for more information.

> Warning

> Security issue: Privileged access gives components access to sensitive data, so permission should be granted carefully, only if you trust a component.

> Note

> This module is complementary to mod_delegation, but can also be used separately.

Available options:

- message: Options
  This option defines permissions for messages. By default no permissions are given. The Options are:

  - outgoing: AccessName
    The option defines an access rule for sending outgoing messages by the component. The default value is none.

- presence: Options
  This option defines permissions for presences. By default no permissions are given. The Options are:

  - managed_entity: AccessName
    An access rule that gives permissions to the component to receive server presences. The default value is none.

  - roster: AccessName
    An access rule that gives permissions to the component to receive the presence of both the users and the contacts in their roster. The default value is none.

- roster: Options
  This option defines roster permissions. By default no permissions are given. The Options are:

  - both: AccessName
    Sets read/write access to a user’s roster. The default value is none.

  - get: AccessName
    Sets read access to a user’s roster. The default value is none.

  - set: AccessName
    Sets write access to a user’s roster. The default value is none.

Example:

    modules:
      mod_privilege:
        roster:
          get: all
        presence:
          managed_entity: all
        message:
          outgoing: all

## mod_proxy65

This module implements XEP-0065: SOCKS5 Bytestreams. It allows ejabberd to act as a file transfer proxy between two XMPP clients.

Available options:

- access: AccessName
  Defines an access rule for file transfer initiators. The default value is all. You may want to restrict access to the users of your server only, in order to avoid abusing your proxy by the users of remote servers.

- auth_type: anonymous | plain
  SOCKS5 authentication type. The default value is anonymous. If set to plain, ejabberd will use authentication backend as it would for SASL PLAIN.

- host
  Deprecated. Use hosts instead.

- hostname: Host
  Defines a hostname offered by the proxy when establishing a session with clients. This is useful when you run the proxy behind a NAT. The keyword @HOST@ is replaced with the virtual host name. The default is to use the value of ip option. Examples: proxy.mydomain.org, 200.150.100.50.

- hosts: [Host, ...]
  This option defines the Jabber IDs of the service. If the hosts option is not specified, the only Jabber ID will be the hostname of the virtual host with the prefix "proxy.". The keyword @HOST@ is replaced with the real virtual host name.

- ip: IPAddress
  This option specifies which network interface to listen for. The default value is an IP address of the service’s DNS name, or, if fails, 127.0.0.1.

- max_connections: pos_integer() | infinity
  Maximum number of active connections per file transfer initiator. The default value is infinity.

- name: Name
  The value of the service name. This name is only visible in some clients that support XEP-0030: Service Discovery. The default is "SOCKS5 Bytestreams".

- port: 1..65535
  A port number to listen for incoming connections. The default value is 7777.

- ram_db_type: mnesia | redis | sql
  Same as top-level default_ram_db option, but applied to this module only.

- recbuf: Size
  A size of the buffer for incoming packets. If you define a shaper, set the value of this option to the size of the shaper in order to avoid traffic spikes in file transfers. The default value is 65536 bytes.

- shaper: Shaper
  This option defines a shaper for the file transfer peers. A shaper with the maximum bandwidth will be selected. The default is none, i.e. no shaper.

- sndbuf: Size
  A size of the buffer for outgoing packets. If you define a shaper, set the value of this option to the size of the shaper in order to avoid traffic spikes in file transfers. The default value is 65536 bytes.

- vcard: vCard
  A custom vCard of the service that will be displayed by some XMPP clients in Service Discovery. The value of vCard is a YAML map constructed from an XML representation of vCard. Since the representation has no attributes, the mapping is straightforward.

Example:

    acl:
      admin:
        user: admin@example.org
      proxy_users:
        server: example.org

    access_rules:
      proxy65_access:
        allow: proxy_users

    shaper_rules:
      proxy65_shaper:
        none: admin
      proxyrate: proxy_users

    shaper:
      proxyrate: 10240

    modules:
      mod_proxy65:
        host: proxy1.example.org
        name: "File Transfer Proxy"
        ip: 200.150.100.1
        port: 7778
        max_connections: 5
        access: proxy65_access
        shaper: proxy65_shaper
        recbuf: 10240
        sndbuf: 10240

## mod_pubsub

This module offers a service for XEP-0060: Publish-Subscribe. The functionality in mod_pubsub can be extended using plugins. The plugin that implements PEP (XEP-0163: Personal Eventing via Pubsub) is enabled in the default ejabberd configuration file, and it requires mod_caps.

Available options:

- access_createnode: AccessName
  This option restricts which users are allowed to create pubsub nodes using acl and access. By default any account in the local ejabberd server is allowed to create pubsub nodes. The default value is: all.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- default_node_config: List of Key:Value
  To override default node configuration, regardless of node plugin. Value is a list of key-value definition. Node configuration still uses default configuration defined by node plugin, and overrides any items by value defined in this configurable list.

- force_node_config: List of Node and the list of its Key:Value
  Define the configuration for given nodes. The default value is: [].

  Example:

      force_node_config:
        ## Avoid buggy clients to make their bookmarks public
        storage:bookmarks:
          access_model: whitelist

- host
  Deprecated. Use hosts instead.

- hosts: [Host, ...]
  This option defines the Jabber IDs of the service. If the hosts option is not specified, the only Jabber ID will be the hostname of the virtual host with the prefix "pubsub.". The keyword @HOST@ is replaced with the real virtual host name.

- ignore_pep_from_offline: false | true
  To specify whether or not we should get last published PEP items from users in our roster which are offline when we connect. Value is true or false. If not defined, pubsub assumes true so we only get last items of online contacts.

- last_item_cache: false | true
  To specify whether or not pubsub should cache last items. Value is true or false. If not defined, pubsub does not cache last items. On systems with not so many nodes, caching last items speeds up pubsub and allows you to raise the user connection rate. The cost is memory usage, as every item is stored in memory.

- max_item_expire_node: timeout() | infinity
  added in 21.12 Specify the maximum item epiry time. Default value is: infinity.

- max_items_node: non_neg_integer() | infinity
  Define the maximum number of items that can be stored in a node. Default value is: 1000.

- max_nodes_discoitems: pos_integer() | infinity
  The maximum number of nodes to return in a discoitem response. The default value is: 100.

- max_subscriptions_node: MaxSubs
  Define the maximum number of subscriptions managed by a node. Default value is no limitation: undefined.

- name: Name
  The value of the service name. This name is only visible in some clients that support XEP-0030: Service Discovery. The default is vCard User Search.

- nodetree: Nodetree
  To specify which nodetree to use. If not defined, the default pubsub nodetree is used: tree. Only one nodetree can be used per host, and is shared by all node plugins.

  - tree nodetree store node configuration and relations on the database. flat nodes are stored without any relationship, and hometree nodes can have child nodes.

  - virtual nodetree does not store nodes on database. This saves resources on systems with tons of nodes. If using the virtual nodetree, you can only enable those node plugins: [flat, pep] or [flat]; any other plugins configuration will not work. Also, all nodes will have the default configuration, and this can not be changed. Using virtual nodetree requires to start from a clean database, it will not work if you used the default tree nodetree before.

- pep_mapping: List of Key:Value
  In this option you can provide a list of key-value to choose defined node plugins on given PEP namespace. The following example will use node_tune instead of node_pep for every PEP node with the tune namespace:

  Example:

      modules:
        ...
        mod_pubsub:
          pep_mapping:
            http://jabber.org/protocol/tune: tune
        ...

- plugins: [Plugin, ...]
  To specify which pubsub node plugins to use. The first one in the list is used by default. If this option is not defined, the default plugins list is: [flat]. PubSub clients can define which plugin to use when creating a node: add type='plugin-name' attribute to the create stanza element.

  - flat plugin handles the default behaviour and follows standard XEP-0060 implementation.

  - pep plugin adds extension to handle Personal Eventing Protocol (XEP-0163) to the PubSub engine. When enabled, PEP is handled automatically.

- vcard: vCard
  A custom vCard of the server that will be displayed by some XMPP clients in Service Discovery. The value of vCard is a YAML map constructed from an XML representation of vCard. Since the representation has no attributes, the mapping is straightforward.

  Example:

      # This XML representation of vCard:
      #   <vCard xmlns='vcard-temp'>
      #     <FN>Conferences</FN>
      #     <ADR>
      #       <WORK/>
      #       <STREET>Elm Street</STREET>
      #     </ADR>
      #   </vCard>
      #
      # is translated to:
      vcard:
        fn: Conferences
        adr:
          -
            work: true
            street: Elm Street

Examples:

Example of configuration that uses flat nodes as default, and allows use of flat, hometree and pep nodes:

    modules:
      mod_pubsub:
        access_createnode: pubsub_createnode
        max_subscriptions_node: 100
        default_node_config:
          notification_type: normal
          notify_retract: false
          max_items: 4
        plugins:
          - flat
          - pep

Using relational database requires using mod_pubsub with db_type sql. Only flat, hometree and pep plugins supports SQL. The following example shows previous configuration with SQL usage:

    modules:
      mod_pubsub:
        db_type: sql
        access_createnode: pubsub_createnode
        ignore_pep_from_offline: true
        last_item_cache: false
        plugins:
          - flat
          - pep

## mod_push

This module implements the XMPP server’s part of the push notification solution specified in XEP-0357: Push Notifications. It does not generate, for example, APNS or FCM notifications directly. Instead, it’s designed to work with so-called "app servers" operated by third-party vendors of mobile apps. Those app servers will usually trigger notification delivery to the user’s mobile device using platform-dependent backend services such as FCM or APNS.

Available options:

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- include_body: true | false | Text
  If this option is set to true, the message text is included with push notifications generated for incoming messages with a body. The option can instead be set to a static Text, in which case the specified text will be included in place of the actual message body. This can be useful to signal the app server whether the notification was triggered by a message with body (as opposed to other types of traffic) without leaking actual message contents. The default value is "New message".

- include_sender: true | false
  If this option is set to true, the sender’s JID is included with push notifications generated for incoming messages with a body. The default value is false.

- notify_on: messages | all
  added in 23.10 If this option is set to messages, notifications are generated only for actual chat messages with a body text (or some encrypted payload). If it’s set to all, any kind of XMPP stanza will trigger a notification. If unsure, it’s strongly recommended to stick to all, which is the default value.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

## mod_push_keepalive

This module tries to keep the stream management session (see mod_stream_mgmt) of a disconnected mobile client alive if the client enabled push notifications for that session. However, the normal session resumption timeout is restored once a push notification is issued, so the session will be closed if the client doesn’t respond to push notifications.

The module depends on mod_push.

Available options:

- resume_timeout: timeout()
  This option specifies the period of time until the session of a disconnected push client times out. This timeout is only in effect as long as no push notification is issued. Once that happened, the resumption timeout configured for mod_stream_mgmt is restored. The default value is 72 hours.

- wake_on_start: true | false
  If this option is set to true, notifications are generated for all registered push clients during server startup. This option should not be enabled on servers with many push clients as it can generate significant load on the involved push services and the server itself. The default value is false.

- wake_on_timeout: true | false
  If this option is set to true, a notification is generated shortly before the session would time out as per the resume_timeout option. The default value is true.

## mod_register

This module adds support for XEP-0077: In-Band Registration. This protocol enables end users to use an XMPP client to:

- Register a new account on the server.

- Change the password from an existing account on the server.

- Delete an existing account on the server.

This module reads also the top-level registration_timeout option defined globally for the server, so please check that option documentation too.

Available options:

- access: AccessName
  Specify rules to restrict what usernames can be registered. If a rule returns deny on the requested username, registration of that user name is denied. There are no restrictions by default.

- access_from: AccessName
  By default, ejabberd doesn’t allow the client to register new accounts from s2s or existing c2s sessions. You can change it by defining access rule in this option. Use with care: allowing registration from s2s leads to uncontrolled massive accounts creation by rogue users.

- access_remove: AccessName
  Specify rules to restrict access for user unregistration. By default any user is able to unregister their account.

- allow_modules: all | [Module, ...]
  added in 21.12 List of modules that can register accounts, or all. The default value is all, which is equivalent to something like [mod_register, mod_register_web].

- captcha_protected: true | false
  Protect registrations with CAPTCHA. The default is false.

- ip_access: AccessName
  Define rules to allow or deny account registration depending on the IP address of the XMPP client. The AccessName should be of type ip. The default value is all.

- password_strength: Entropy
  This option sets the minimum Shannon entropy for passwords. The value Entropy is a number of bits of entropy. The recommended minimum is 32 bits. The default is 0, i.e. no checks are performed.

- redirect_url: URL
  This option enables registration redirection as described in XEP-0077: In-Band Registration: Redirection.

- registration_watchers: [JID, ...]
  This option defines a list of JIDs which will be notified each time a new account is registered.

- welcome_message: {subject: Subject, body: Body}
  Set a welcome message that is sent to each newly registered account. The message will have subject Subject and text Body.

  Example:

      modules:
        mod_register:
          welcome_message:
            subject: "Welcome!"
            body: |-
              Hi!
              Welcome to this XMPP server

## mod_register_web

This module provides a web page where users can:

- Register a new account on the server.

- Change the password from an existing account on the server.

- Unregister an existing account on the server.

This module supports CAPTCHA to register a new account. To enable this feature, configure the top-level captcha_cmd and top-level captcha_url options.

As an example usage, the users of the host localhost can visit the page: https://localhost:5280/register/ It is important to include the last / character in the URL, otherwise the subpages URL will be incorrect.

This module is enabled in listen → ejabberd_http → request_handlers, no need to enable in modules. The module depends on mod_register where all the configuration is performed.

The module has no options.

Example:

    listen:
      -
        port: 5280
        module: ejabberd_http
        request_handlers:
          /register: mod_register_web

    modules:
      mod_register: {}

## mod_roster

This module implements roster management as defined in RFC6121 Section 2. The module also adds support for XEP-0237: Roster Versioning.

Available options:

- access: AccessName
  This option can be configured to specify rules to restrict roster management. If the rule returns deny on the requested user name, that user cannot modify their personal roster, i.e. they cannot add/remove/modify contacts or send presence subscriptions. The default value is all, i.e. no restrictions.

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- store_current_id: true | false
  If this option is set to true, the current roster version number is stored on the database. If set to false, the roster version number is calculated on the fly each time. Enabling this option reduces the load for both ejabberd and the database. This option does not affect the client in any way. This option is only useful if option versioning is set to true. The default value is false. IMPORTANT: if you use mod_shared_roster or mod_shared_roster_ldap, you must set the value of the option to false.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

- versioning: true | false
  Enables/disables Roster Versioning. The default value is false.

Example:

    modules:
      mod_roster:
        versioning: true
        store_current_id: false

## mod_s2s_dialback

The module adds support for XEP-0220: Server Dialback to provide server identity verification based on DNS.

> Warning

> DNS-based verification is vulnerable to DNS cache poisoning, so modern servers rely on verification based on PKIX certificates. Thus this module is only recommended for backward compatibility with servers running outdated software or non-TLS servers, or those with invalid certificates (as long as you accept the risks, e.g. you assume that the remote server has an invalid certificate due to poor administration and not because it’s compromised).

Available options:

- access: AccessName
  An access rule that can be used to restrict dialback for some servers. The default value is all.

Example:

    modules:
      mod_s2s_dialback:
        access:
          allow:
            server: legacy.domain.tld
            server: invalid-cert.example.org
          deny: all

## mod_service_log

This module forwards copies of all stanzas to remote XMPP servers or components. Every stanza is encapsulated into <forwarded/> element as described in XEP-0297: Stanza Forwarding.

Available options:

- loggers: [Domain, ...]
  A list of servers or connected components to which stanzas will be forwarded.

Example:

    modules:
      mod_service_log:
        loggers:
          - xmpp-server.tld
          - component.domain.tld

## mod_shared_roster

This module enables you to create shared roster groups: groups of accounts that can see members from (other) groups in their rosters.

The big advantages of this feature are that end users do not need to manually add all users to their rosters, and that they cannot permanently delete users from the shared roster groups. A shared roster group can have members from any XMPP server, but the presence will only be available from and to members of the same virtual host where the group is created. It still allows the users to have / add their own contacts, as it does not replace the standard roster. Instead, the shared roster contacts are merged to the relevant users at retrieval time. The standard user rosters thus stay unmodified.

Shared roster groups can be edited via the Web Admin, and some API commands called srg_*. Each group has a unique name and those parameters:

- Label: Used in the rosters where this group is displayed.

- Description: of the group, which has no effect.

- Members: A list of JIDs of group members, entered one per line in the Web Admin. The special member directive @all@ represents all the registered users in the virtual host; which is only recommended for a small server with just a few hundred users. The special member directive @online@ represents the online users in the virtual host. With those two directives, the actual list of members in those shared rosters is generated dynamically at retrieval time.

- Displayed: A list of groups that will be in the rosters of this group’s members. A group of other vhost can be identified with groupid@vhost.

This module depends on mod_roster. If not enabled, roster queries will return 503 errors.

Available options:

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql
  Same as top-level default_db option, but applied to this module only.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

Examples:

Take the case of a computer club that wants all its members seeing each other in their rosters. To achieve this, they need to create a shared roster group similar to this one:

    Name: club_members
    Label: Club Members
    Description: Members from the computer club
    Members: member1@example.org, member2@example.org, member3@example.org
    Displayed Groups: club_members

In another case we have a company which has three divisions: Management, Marketing and Sales. All group members should see all other members in their rosters. Additionally, all managers should have all marketing and sales people in their roster. Simultaneously, all marketeers and the whole sales team should see all managers. This scenario can be achieved by creating shared roster groups as shown in the following lists:

    First list:
    Name: management
    Label: Management
    Description: Management
    Members: manager1@example.org, manager2@example.org
    Displayed: management, marketing, sales

    Second list:
    Name: marketing
    Label: Marketing
    Description: Marketing
    Members: marketeer1@example.org, marketeer2@example.org, marketeer3@example.org
    Displayed: management, marketing

    Third list:
    Name: sales
    Label: Sales
    Description: Sales
    Members: salesman1@example.org, salesman2@example.org, salesman3@example.org
    Displayed: management, sales

## mod_shared_roster_ldap

This module lets the server administrator automatically populate users' rosters (contact lists) with entries based on users and groups defined in an LDAP-based directory.

> Note

> mod_shared_roster_ldap depends on mod_roster being enabled. Roster queries will return 503 errors if mod_roster is not enabled.

The module accepts many configuration options. Some of them, if unspecified, default to the values specified for the top level of configuration. This lets you avoid specifying, for example, the bind password in multiple places.

- Filters: ldap_rfilter, ldap_ufilter, ldap_gfilter, ldap_filter. These options specify LDAP filters used to query for shared roster information. All of them are run against the ldap_base.

- Attributes: ldap_groupattr, ldap_groupdesc, ldap_memberattr, ldap_userdesc, ldap_useruid. These options specify the names of the attributes which hold interesting data in the entries returned by running filters specified with the filter options.

- Control parameters: ldap_auth_check, ldap_group_cache_validity, ldap_memberattr_format, ldap_memberattr_format_re, ldap_user_cache_validity. These parameters control the behaviour of the module.

- Connection parameters: The module also accepts the connection parameters, all of which default to the top-level parameter of the same name, if unspecified. See LDAP Connection section for more information about them.

Check also the Configuration examples section to get details about retrieving the roster, and configuration examples including Flat DIT and Deep DIT.

Available options:

- cache_life_time
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed
  Same as top-level cache_missed option, but applied to this module only.

- cache_size
  Same as top-level cache_size option, but applied to this module only.

- ldap_auth_check: true | false
  Whether the module should check (via the ejabberd authentication subsystem) for existence of each user in the shared LDAP roster. Set to false if you want to disable the check. Default value is true.

- ldap_backups
  Same as top-level ldap_backups option, but applied to this module only.

- ldap_base
  Same as top-level ldap_base option, but applied to this module only.

- ldap_deref_aliases
  Same as top-level ldap_deref_aliases option, but applied to this module only.

- ldap_encrypt
  Same as top-level ldap_encrypt option, but applied to this module only.

- ldap_filter
  Additional filter which is AND-ed together with "User Filter" and "Group Filter". For more information check the LDAP Filters section.

- ldap_gfilter
  "Group Filter", used when retrieving human-readable name (a.k.a. "Display Name") and the members of a group. See also the parameters ldap_groupattr, ldap_groupdesc and ldap_memberattr. If unspecified, defaults to the top-level parameter of the same name. If that one also is unspecified, then the filter is constructed exactly like "User Filter".

- ldap_groupattr
  The name of the attribute that holds the group name, and that is used to differentiate between them. Retrieved from results of the "Roster Filter" and "Group Filter". Defaults to cn.

- ldap_groupdesc
  The name of the attribute which holds the human-readable group name in the objects you use to represent groups. Retrieved from results of the "Group Filter". Defaults to whatever ldap_groupattr is set.

- ldap_memberattr
  The name of the attribute which holds the IDs of the members of a group. Retrieved from results of the "Group Filter". Defaults to memberUid. The name of the attribute differs depending on the objectClass you use for your group objects, for example: posixGroup → memberUid; groupOfNames → member; groupOfUniqueNames → uniqueMember.

- ldap_memberattr_format
  A globbing format for extracting user ID from the value of the attribute named by ldap_memberattr. Defaults to %u, which means that the whole value is the member ID. If you change it to something different, you may also need to specify the User and Group Filters manually; see section Filters.

- ldap_memberattr_format_re
  A regex for extracting user ID from the value of the attribute named by ldap_memberattr. Check the LDAP Control Parameters section.

- ldap_password
  Same as top-level ldap_password option, but applied to this module only.

- ldap_port
  Same as top-level ldap_port option, but applied to this module only.

- ldap_rfilter
  So called "Roster Filter". Used to find names of all "shared roster" groups. See also the ldap_groupattr parameter. If unspecified, defaults to the top-level parameter of the same name. You must specify it in some place in the configuration, there is no default.

- ldap_rootdn
  Same as top-level ldap_rootdn option, but applied to this module only.

- ldap_servers
  Same as top-level ldap_servers option, but applied to this module only.

- ldap_tls_cacertfile
  Same as top-level ldap_tls_cacertfile option, but applied to this module only.

- ldap_tls_certfile
  Same as top-level ldap_tls_certfile option, but applied to this module only.

- ldap_tls_depth
  Same as top-level ldap_tls_depth option, but applied to this module only.

- ldap_tls_verify
  Same as top-level ldap_tls_verify option, but applied to this module only.

- ldap_ufilter
  "User Filter", used for retrieving the human-readable name of roster entries (usually full names of people in the roster). See also the parameters ldap_userdesc and ldap_useruid. For more information check the LDAP Filters section.

- ldap_uids
  Same as top-level ldap_uids option, but applied to this module only.

- ldap_userdesc
  The name of the attribute which holds the human-readable user name. Retrieved from results of the "User Filter". Defaults to cn.

- ldap_userjidattr
  The name of the attribute which is used to map user id to XMPP jid. If not specified (and that is default value of this option), user jid will be created from user id and this module host.

- ldap_useruid
  The name of the attribute which holds the ID of a roster item. Value of this attribute in the roster item objects needs to match the ID retrieved from the ldap_memberattr attribute of a group object. Retrieved from results of the "User Filter". Defaults to cn.

- use_cache
  Same as top-level use_cache option, but applied to this module only.

## mod_sic

This module adds support for XEP-0279: Server IP Check. This protocol enables a client to discover its external IP address.

> Warning

> The protocol extension is deferred and seems like there are no clients supporting it, so using this module is not recommended and, furthermore, the module might be removed in the future.

The module has no options.

## mod_sip

This module adds SIP proxy/registrar support for the corresponding virtual host.

> Note

> It is not enough to just load this module. You should also configure listeners and DNS records properly. For details see the section about the ejabberd_sip listen module in the ejabberd Documentation.

Available options:

- always_record_route: true | false
  Always insert "Record-Route" header into SIP messages. With this approach it is possible to bypass NATs/firewalls a bit more easily. The default value is true.

- flow_timeout_tcp: timeout()
  The option sets a keep-alive timer for SIP outbound TCP connections. The default value is 2 minutes.

- flow_timeout_udp: timeout()
  The options sets a keep-alive timer for SIP outbound UDP connections. The default value is 29 seconds.

- record_route: URI
  When the option always_record_route is set to true or when SIP outbound is utilized, ejabberd inserts "Record-Route" header field with this URI into a SIP message. The default is a SIP URI constructed from the virtual host on which the module is loaded.

- routes: [URI, ...]
  You can set a list of SIP URIs of routes pointing to this SIP proxy server. The default is a list containing a single SIP URI constructed from the virtual host on which the module is loaded.

- via: [URI, ...]
  A list to construct "Via" headers for inserting them into outgoing SIP messages. This is useful if you’re running your SIP proxy in a non-standard network topology. Every URI element in the list must be in the form of "scheme://host:port", where "transport" must be tls, tcp, or udp, "host" must be a domain name or an IP address and "port" must be an internet port number. Note that all parts of the URI are mandatory (e.g. you cannot omit "port" or "scheme").

Example:

    modules:
      mod_sip:
        always_record_route: false
        record_route: "sip:example.com;lr"
        routes:
          - "sip:example.com;lr"
          - "sip:sip.example.com;lr"
        flow_timeout_udp: 30 sec
        flow_timeout_tcp: 1 min
        via:
          - tls://sip-tls.example.com:5061
          - tcp://sip-tcp.example.com:5060
          - udp://sip-udp.example.com:5060

## mod_stats

This module adds support for XEP-0039: Statistics Gathering. This protocol allows you to retrieve the following statistics from your ejabberd server:

- Total number of registered users on the current virtual host (users/total).

- Total number of registered users on all virtual hosts (users/all-hosts/total).

- Total number of online users on the current virtual host (users/online).

- Total number of online users on all virtual hosts (users/all-hosts/online).

> Note

> The protocol extension is deferred and seems like even a few clients that were supporting it are now abandoned. So using this module makes very little sense.

The module has no options.

## mod_stream_mgmt

This module adds support for XEP-0198: Stream Management. This protocol allows active management of an XML stream between two XMPP entities, including features for stanza acknowledgments and stream resumption.

Available options:

- ack_timeout: timeout()
  A time to wait for stanza acknowledgments. Setting it to infinity effectively disables the timeout. The default value is 1 minute.

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only. The default value is 48 hours.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- max_ack_queue: Size
  This option specifies the maximum number of unacknowledged stanzas queued for possible retransmission. When the limit is exceeded, the client session is terminated. The allowed values are positive integers and infinity. You should be careful when setting this value as it should not be set too low, otherwise, you could kill sessions in a loop, before they get the chance to finish proper session initiation. It should definitely be set higher that the size of the offline queue (for example at least 3 times the value of the max offline queue and never lower than 1000). The default value is 5000.

- max_resume_timeout: timeout()
  A client may specify the period of time until a session times out if the connection is lost. During this period of time, the client may resume its session. This option limits the period of time a client is permitted to request. It must be set to a timeout equal to or larger than the default resume_timeout. By default, it is set to the same value as the resume_timeout option.

- queue_type: ram | file
  Same as top-level queue_type option, but applied to this module only.

- resend_on_timeout: true | false | if_offline
  If this option is set to true, any message stanzas that weren’t acknowledged by the client will be resent on session timeout. This behavior might often be desired, but could have unexpected results under certain circumstances. For example, a message that was sent to two resources might get resent to one of them if the other one timed out. Therefore, the default value for this option is false, which tells ejabberd to generate an error message instead. As an alternative, the option may be set to if_offline. In this case, unacknowledged messages are resent only if no other resource is online when the session times out. Otherwise, error messages are generated.

- resume_timeout: timeout()
  This option configures the (default) period of time until a session times out if the connection is lost. During this period of time, a client may resume its session. Note that the client may request a different timeout value, see the max_resume_timeout option. Setting it to 0 effectively disables session resumption. The default value is 5 minutes.

## mod_stun_disco

added in 20.04

This module allows XMPP clients to discover STUN/TURN services and to obtain temporary credentials for using them as per XEP-0215: External Service Discovery.

Available options:

- access: AccessName
  This option defines which access rule will be used to control who is allowed to discover STUN/TURN services and to request temporary credentials. The default value is local.

- credentials_lifetime: timeout()
  The lifetime of temporary credentials offered to clients. If ejabberd’s built-in TURN service is used, TURN relays allocated using temporary credentials will be terminated shortly after the credentials expired. The default value is 12 hours. Note that restarting the ejabberd node invalidates any temporary credentials offered before the restart unless a secret is specified (see below).

- offer_local_services: true | false
  This option specifies whether local STUN/TURN services configured as ejabberd listeners should be announced automatically. Note that this will not include TLS-enabled services, which must be configured manually using the services option (see below). For non-anonymous TURN services, temporary credentials will be offered to the client. The default value is true.

- secret: Text
  The secret used for generating temporary credentials. If this option isn’t specified, a secret will be auto-generated. However, a secret must be specified explicitly if non-anonymous TURN services running on other ejabberd nodes and/or external TURN services are configured. Also note that auto-generated secrets are lost when the node is restarted, which invalidates any credentials offered before the restart. Therefore, it’s recommended to explicitly specify a secret if clients cache retrieved credentials (for later use) across service restarts.

- services: [Service, ...]
  The list of services offered to clients. This list can include STUN/TURN services running on any ejabberd node and/or external services. However, if any listed TURN service not running on the local ejabberd node requires authentication, a secret must be specified explicitly, and must be shared with that service. This will only work with ejabberd’s built-in STUN/TURN server and with external servers that support the same REST API For Access To TURN Services. Unless the offer_local_services is set to false, the explicitly listed services will be offered in addition to those announced automatically.

  - host: Host
    The hostname or IP address the STUN/TURN service is listening on. For non-TLS services, it’s recommended to specify an IP address (to avoid additional DNS lookup latency on the client side). For TLS services, the hostname (or IP address) should match the certificate. Specifying the host option is mandatory.

  - port: 1..65535
    The port number the STUN/TURN service is listening on. The default port number is 3478 for non-TLS services and 5349 for TLS services.

  - restricted: true | false
    This option determines whether temporary credentials for accessing the service are offered. The default is false for STUN/STUNS services and true for TURN/TURNS services.

  - transport: tcp | udp
    The transport protocol supported by the service. The default is udp for non-TLS services and tcp for TLS services.

  - type: stun | turn | stuns | turns
    The type of service. Must be stun or turn for non-TLS services, stuns or turns for TLS services. The default type is stun.

  Example:

      services:
        -
          host: 203.0.113.3
          port: 3478
          type: stun
          transport: udp
          restricted: false
        -
          host: 203.0.113.3
          port: 3478
          type: turn
          transport: udp
          restricted: true
        -
          host: 2001:db8::3
          port: 3478
          type: stun
          transport: udp
          restricted: false
        -
          host: 2001:db8::3
          port: 3478
          type: turn
          transport: udp
          restricted: true
        -
          host: server.example.com
          port: 5349
          type: turns
          transport: tcp
          restricted: true

## mod_time

This module adds support for XEP-0202: Entity Time. In other words, the module reports server’s system time.

The module has no options.

## mod_vcard

This module allows end users to store and retrieve their vCard, and to retrieve other users vCards, as defined in XEP-0054: vcard-temp. The module also implements an uncomplicated Jabber User Directory based on the vCards of these users. Moreover, it enables the server to send its vCard when queried.

Available options:

- allow_return_all: true | false
  This option enables you to specify if search operations with empty input fields should return all users who added some information to their vCard. The default value is false.

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- db_type: mnesia | sql | ldap
  Same as top-level default_db option, but applied to this module only.

- host
  Deprecated. Use hosts instead.

- hosts: [Host, ...]
  This option defines the Jabber IDs of the service. If the hosts option is not specified, the only Jabber ID will be the hostname of the virtual host with the prefix "vjud.". The keyword @HOST@ is replaced with the real virtual host name.

- matches: pos_integer() | infinity
  With this option, the number of reported search results can be limited. If the option’s value is set to infinity, all search results are reported. The default value is 30.

- name: Name
  The value of the service name. This name is only visible in some clients that support XEP-0030: Service Discovery. The default is vCard User Search.

- search: true | false
  This option specifies whether the search functionality is enabled or not. If disabled, the options hosts, name and vcard will be ignored and the Jabber User Directory service will not appear in the Service Discovery item list. The default value is false.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

- vcard: vCard
  A custom vCard of the server that will be displayed by some XMPP clients in Service Discovery. The value of vCard is a YAML map constructed from an XML representation of vCard. Since the representation has no attributes, the mapping is straightforward.

  Example:

      # This XML representation of vCard:
      #
      #   <vCard xmlns='vcard-temp'>
      #     <FN>Conferences</FN>
      #     <ADR>
      #       <WORK/>
      #       <STREET>Elm Street</STREET>
      #     </ADR>
      #   </vCard>
      #
      # is translated to:
      #
      vcard:
        fn: Conferences
        adr:
          -
            work: true
            street: Elm Street

Available options for ldap backend:

- ldap_backups
  Same as top-level ldap_backups option, but applied to this module only.

- ldap_base
  Same as top-level ldap_base option, but applied to this module only.

- ldap_deref_aliases
  Same as top-level ldap_deref_aliases option, but applied to this module only.

- ldap_encrypt
  Same as top-level ldap_encrypt option, but applied to this module only.

- ldap_filter
  Same as top-level ldap_filter option, but applied to this module only.

- ldap_password
  Same as top-level ldap_password option, but applied to this module only.

- ldap_port
  Same as top-level ldap_port option, but applied to this module only.

- ldap_rootdn
  Same as top-level ldap_rootdn option, but applied to this module only.

- ldap_search_fields: {Name: Attribute, ...}
  This option defines the search form and the LDAP attributes to search within. Name is the name of a search form field which will be automatically translated by using the translation files (see msgs/*.msg for available words). Attribute is the LDAP attribute or the pattern %u.

  Examples:

  The default is:

      User: "%u"
      "Full Name": displayName
      "Given Name": givenName
      "Middle Name": initials
      "Family Name": sn
      Nickname: "%u"
      Birthday: birthDay
      Country: c
      City: l
      Email: mail
      "Organization Name": o
      "Organization Unit": ou

- ldap_search_reported: {SearchField: VcardField}, ...}
  This option defines which search fields should be reported. SearchField is the name of a search form field which will be automatically translated by using the translation files (see msgs/*.msg for available words). VcardField is the vCard field name defined in the ldap_vcard_map option.

  Examples:

  The default is:

      "Full Name": FN
      "Given Name": FIRST
      "Middle Name": MIDDLE
      "Family Name": LAST
      "Nickname": NICKNAME
      "Birthday": BDAY
      "Country": CTRY
      "City": LOCALITY
      "Email": EMAIL
      "Organization Name": ORGNAME
      "Organization Unit": ORGUNIT

- ldap_servers
  Same as top-level ldap_servers option, but applied to this module only.

- ldap_tls_cacertfile
  Same as top-level ldap_tls_cacertfile option, but applied to this module only.

- ldap_tls_certfile
  Same as top-level ldap_tls_certfile option, but applied to this module only.

- ldap_tls_depth
  Same as top-level ldap_tls_depth option, but applied to this module only.

- ldap_tls_verify
  Same as top-level ldap_tls_verify option, but applied to this module only.

- ldap_uids
  Same as top-level ldap_uids option, but applied to this module only.

- ldap_vcard_map: {Name: {Pattern, LDAPattributes}, ...}
  With this option you can set the table that maps LDAP attributes to vCard fields. Name is the type name of the vCard as defined in RFC 2426. Pattern is a string which contains pattern variables %u, %d or %s. LDAPattributes is the list containing LDAP attributes. The pattern variables %s will be sequentially replaced with the values of LDAP attributes from List_of_LDAP_attributes, %u will be replaced with the user part of a JID, and %d will be replaced with the domain part of a JID.

  Examples:

  The default is:

      NICKNAME: {"%u": []}
      FN: {"%s": [displayName]}
      LAST: {"%s": [sn]}
      FIRST: {"%s": [givenName]}
      MIDDLE: {"%s": [initials]}
      ORGNAME: {"%s": [o]}
      ORGUNIT: {"%s": [ou]}
      CTRY: {"%s": [c]}
      LOCALITY: {"%s": [l]}
      STREET: {"%s": [street]}
      REGION: {"%s": [st]}
      PCODE: {"%s": [postalCode]}
      TITLE: {"%s": [title]}
      URL: {"%s": [labeleduri]}
      DESC: {"%s": [description]}
      TEL: {"%s": [telephoneNumber]}
      EMAIL: {"%s": [mail]}
      BDAY: {"%s": [birthDay]}
      ROLE: {"%s": [employeeType]}
      PHOTO: {"%s": [jpegPhoto]}

Available options for mnesia backend:

- search_all_hosts: true | false
  Whether to perform search on all virtual hosts or not. The default value is true.

## mod_vcard_xupdate

The user’s client can store an avatar in the user vCard. The vCard-Based Avatars protocol (XEP-0153) provides a method for clients to inform the contacts what is the avatar hash value. However, simple or small clients may not implement that protocol.

If this module is enabled, all the outgoing client presence stanzas get automatically the avatar hash on behalf of the client. So, the contacts receive the presence stanzas with the Update Data described in XEP-0153 as if the client would had inserted it itself. If the client had already included such element in the presence stanza, it is replaced with the element generated by ejabberd.

By enabling this module, each vCard modification produces a hash recalculation, and each presence sent by a client produces hash retrieval and a presence stanza rewrite. For this reason, enabling this module will introduce a computational overhead in servers with clients that change frequently their presence. However, the overhead is significantly reduced by the use of caching, so you probably don’t want to set use_cache to false.

The module depends on mod_vcard.

> Note

> Nowadays XEP-0153 is used mostly as "read-only", i.e. modern clients don’t publish their avatars inside vCards. Thus in the majority of cases the module is only used along with mod_avatar for providing backward compatibility.

Available options:

- cache_life_time: timeout()
  Same as top-level cache_life_time option, but applied to this module only.

- cache_missed: true | false
  Same as top-level cache_missed option, but applied to this module only.

- cache_size: pos_integer() | infinity
  Same as top-level cache_size option, but applied to this module only.

- use_cache: true | false
  Same as top-level use_cache option, but applied to this module only.

## mod_version

This module implements XEP-0092: Software Version. Consequently, it answers ejabberd’s version when queried.

Available options:

- show_os: true | false
  Should the operating system be revealed or not. The default value is true.